HoskoteConstruction
Balaji Gold City, Hoskote, Bengaluru Rural, Karnataka – 562114  |  UDYAM-KR-02-0127051  |  +91 97428 01802
DETAILED COST ESTIMATE (BILL OF QUANTITIES)
Proposed for Residential Building at: ______________________________________________
In favour of: ______________________________  |  Date: ____________
	Sl No
	Particulars
	Unit
	Qty
	Rate (₹)
	Amount (₹)

	1. EARTHWORK

	1.01
	General excavation (all soil types) up to 3.00m depth, incl. backfilling, dewatering, disposal
	Cum
	90
	1,500
	1,35,000

	
	SUB TOTAL — EARTHWORK
	
	
	
	1,35,000

	2. CONCRETE

	2.01
	PCC 1:3:6, 20mm & down aggregate, incl. base prep, compaction, curing
	Cum
	14
	6,000
	84,000

	2.02
	RMC/M25 Grade — Columns (below GF, GF, First Floor)
	Cum
	19
	6,000
	1,14,000

	2.03
	RMC/M25 Grade — Slab (Ground Floor, First Floor)
	Cum
	36
	6,000
	2,16,000

	2.04
	RMC/M25 Grade — Beams (Plinth, GF, First Floor)
	Cum
	24
	6,000
	1,44,000

	2.05
	Footing / raft slab for columns & retaining walls
	Cum
	14
	6,000
	84,000

	2.06
	Staircase, lintels, chajja/lofts (all floors)
	Cum
	34
	6,000
	2,04,000

	
	SUB TOTAL — CONCRETE
	
	
	
	8,46,000

	3. FORM WORK (Shuttering)

	3.01
	Columns — below GF, GF, First Floor
	Sqm
	90
	1,400
	1,26,000

	3.02
	Slab — Ground Floor, First Floor
	Sqm
	190
	1,400
	2,66,000

	3.03
	Beams — Plinth, GF, First Floor
	Sqm
	235
	1,400
	3,29,000

	3.04
	Footing/raft slab, retaining walls, ramp, staircase & misc.
	Sqm
	165
	1,400
	2,30,000

	
	SUB TOTAL — FORM WORK
	
	
	
	9,51,000

	4. STEEL

	4.01
	Fe500 HSD reinforcement steel — fabrication & fixing as per drawings
	Ton
	10
	61,000
	6,10,000

	
	SUB TOTAL — STEEL
	
	
	
	6,10,000

	5. MASONRY

	5.01
	Size stone masonry in foundation & plinth, CM 1:4
	Cum
	25
	5,600
	1,40,000

	5.02
	Table-moulded burnt brick masonry, 230mm, CM 1:6, superstructure
	Cum
	120
	5,600
	6,72,000

	
	SUB TOTAL — MASONRY
	
	
	
	8,12,000

	6. PLASTERING

	6.01
	External plastering, 2 coats CM 1:6 with waterproof compound, sand-faced finish
	Sqm
	280
	3,700
	10,36,000

	
	SUB TOTAL — PLASTERING
	
	
	
	10,36,000

	7. PAINTING

	7.01
	External textured paint, approved make/shade, base coat + 2 finish coats
	Sqm
	280
	2,600
	7,28,000

	
	SUB TOTAL — PAINTING
	
	
	
	7,28,000

	8. DOORS & WINDOWS

	8.01
	Teak panelled single-shutter door, teakwood frame 75x125mm, incl. hardware
	Sqm
	10
	7,400
	74,000

	
	SUB TOTAL — DOORS & WINDOWS
	
	
	
	74,000

	9. FLOORING / DADOING

	9.01
	Vitrified tile flooring 600x600mm over 20mm CM 1:4 bed, incl. grouting
	Sqm
	125
	2,400
	3,00,000

	9.02
	Vitrified tile skirting, 100mm high, matching grout
	Rmt
	34
	1,200
	40,800

	
	SUB TOTAL — FLOORING & DADOING
	
	
	
	3,40,800

	10. MISCELLANEOUS

	10.01
	PVC rainwater downpipe (SWR) 100mm dia, incl. fittings & brackets
	Rmt
	14
	1,400
	19,600

	10.02
	Terrace waterproofing, surface method, 10-year guarantee spec
	Sqm
	48
	2,400
	1,15,200

	10.03
	Toilet waterproofing, 2-layer surface method, 10-year guarantee spec
	Sqm
	10
	1,400
	14,000

	10.04
	UG sump tank — RCC M20, incl. excavation, steel, waterproofing
	Ltrs
	8000
	15
	1,20,000

	10.05
	Overhead Sintex tank incl. platform
	Ltrs
	2000
	24
	48,000

	10.06
	Compound wall, 150mm hollow block masonry, incl. foundation, plaster, MS gates
	Rmt
	56
	3,200
	1,79,200

	10.07
	Flagging/apron concrete around building, PCC 1:4:8, 100mm thick
	Sqm
	9
	6,000
	54,000

	10.08
	CI manhole frame & cover for UG sump
	Nos
	9
	3,200
	28,800

	
	SUB TOTAL — MISCELLANEOUS
	
	
	
	5,78,800

	
	SUB TOTAL — CIVIL WORKS (1–10)
	
	
	
	61,11,600

	11
	Electrification (7% of civil works total)
	—
	—
	—
	4,27,812

	12
	Plumbing (7% of civil works total)
	—
	—
	—
	4,27,812

	
	GRAND TOTAL (A) — Civil, Electrical & Plumbing
	
	
	
	69,67,224



Part B — Interiors & Fittings (Optional Add-on)
	Sl No
	Particulars
	Unit
	Qty
	Rate (₹)
	Amount (₹)

	1
	Wardrobes — 19mm BWP plywood, laminate finish, SS hinges, drawers with lock
	Sft
	120
	1,350
	1,62,000

	2
	TV unit — box-type cabinet, 450mm depth, laminate finish
	Sft
	45
	950
	42,750

	3
	Kitchen cabinet bottom unit — 19mm BWP plywood, auto-loaded hinges
	Sft
	30
	1,980
	59,400

	4
	Kitchen overhead/middle unit — 19mm BWP plywood, laminate finish
	Sft
	14
	1,100
	15,400

	5
	Full-height storage & loft unit
	Sft
	50
	875
	43,750

	6
	Pooja unit — as per design
	Sft
	45
	850
	38,250

	7
	False ceiling — gypsum board, Saint-Gobain Gyproc system
	Sft
	500
	75
	37,500

	
	ESTIMATED TOTAL (B) — Interiors
	
	
	
	3,99,050

	
	TOTAL (A + B)
	
	
	
	73,66,274



Note: Rates shown are illustrative market rates for reference and should be updated to current rates before submission. This estimate covers civil, electrical, plumbing, and optional interior works as itemised above. For bank loan submission, this estimate is typically accompanied by the Panchayat/BMRDA-approved building plan and a construction agreement.

Prepared by: HoskoteConstruction
Certified by: _______________________ (Civil Engineer, Name & License No.)
